How many Fast Ethernet interfaces does the switch have?

0/1

How many Gigabit Ethernet interfaces does the switch have?

2

What is the range of values shown for the vty lines?

0 4 / 5 15

Which command will display the current contents of non-volatile random-access memory (NVRAM)?

Why does the switch respond with “startup-config is not present?”

Why is the **login** command required?

enable password authentication for console access